**Security Script for future use:**

hostname MLS5

!

enable secret cisco

!

banner motd #No unauthorized access allowed!#

!

line con 0

exec-timeout 5 0

password 7 0822455D0A16

login

!

line vty 0 4

password 7 0822455D0A16

login

transport input telnet

!

service password-encryption

!